HTD8808 LCD Digital Non-Contact IR Infrared Laser Body Forehead Thermometer Temp Gun

New Digital LCD Non-Contact IR Infrared Laser Body Forehead Thermometer Temp Gun

HTD8808 Non-Contact Digital Infrared Forehead Food Body Thermometer Temperature Meter

Non-Contact IR Laser Temp Gun Infrared Digital Thermometer Baby Kids Body Temperature Tester

Description:

•100% Brand New.

•Size:150x95x44mm(LxWxH)

•Multiple function: Not only can measure body temperature, but also can measure the temperature of surface, room, bath water, food, baby milk etc. with clock function.

•Fast and accurate:0.5 seconds measuring time and the accuracy is ±0.2C(0.4F)

•Non contact: safe and clean, 5-15cm(2-5.9inch) measuring distance.

•Easy to use: Operate with one button, very simple to use.

•Three color backlight (color alarm): When the body temperature is normal, the backlight is Green, Yellow backlight for slight fever and Red backlight for high fever.

•Large memories: can store 50 memories for data analysis.

•Alarm value can be set.

•C and F be changeable and selectable.

•Auto shut off: 5 seconds without operation.

•Setting can be adjusted for different kinds of people (such as white people , black people, yellow people etc.)

•Display resolution is 0.1C(0.1F)

•Buzzer can be closed or opened by manual

•Bluetooth wireless communication (Optional): Can be connected to data analysis systems.

•Voice function (Optional): Can be added according to client's requirement.

•Note: the alarm point is settable, The Red backlight is object to the alarm point, onece the temperature is above the alarm point, the backlight is RED, if the alarm point is below 37.5°C(99.5°F), there is no yellow backlight ,only Green and RED backlight.

Specifications:

Model: HTD8808

Dimensions : approx.15 x 8.4 x 4.3cm

Resolution: ±0.1°C/±0.1°F

Three color back light (color alarm):

32~37.5°C(89.6~99.5°F):Green back-light (Normal)

37.6~38.0°C(Alarm point)(99.7°F-100.4°F):yellow back-light( slight fever)

38.1-42.9°C(100.6°F-109.2°F):Red back-light (High fever)

Note: Three-color back-light is only for body mode, Always Green back-light for surface mode.

Measuring range:

Body mode:32-42.9°C(89.6~109.2°F)

surface mode:0~100°C(32-212°F)

Measuring time : 0.5 seconds

Auto shut off : 5 seconds

Operating conditions : 5°C-40.0°C(41°F-104.0°F),Rh≤85%

Battery: 2 x 1.5V AAA battery (battery NOT Included)

Package:

1x Non-contact Infrared body Thermometer (batteries are not included)

1x English Manual