Digital Thermometer & Hygrometer Combined Gauge With Remote Probe Indoor Outdoor

Indoor/ Outdoor Thermometer Hygrometer Temperature Humidity Meter With Remote Probe

LCD Digital Indoor Outdoor Temperature Meter Thermometer Hygrometer Humidity Gauge With probe

Digital LCD Thermometer Temperature Meter Indoor Outdoor Clock with Romete Probe

Features:

For precise supervision of the temperature and air humidity in terrariums or other applications as required.

The unit will show the temperature at the remote probe (OUT) and at gauge (IN).

The readout can be switched using the IN/OUT button function.

The Max/Min button function will show the maximum or minimum temperatures at either the gauge or remote probe.

The humidity level is measured using the remote humidity probe.

Each external probe has cable length of 36” (900mm) with suction cup.

Stores maximum and minimum temperatures.

Technical Information:

Indoor Temperature Range：-10C-50C (14F-122F)

Outdoor Temperature Range:- -50-+70C（-58F~158F）

Outdoor Humidity Measuring Range:-10-95%RH

Unit Size:- 63x63x12mm

Uses AAA batteries (Not Supplied)

Clip out arm for a free standing unit

Package content:

1 x Thermometer & Hygrometer

1 x User manual