Digital LCD Indoor Thermometer Hygrometer Alarm Clock Temperature Humidity Meter

Digital LCD Indoor Thermometer Hygrometer Temperature Humidity Meter Gauge With Alarm Clock

Digital Indoor LCD Alarm Clock Thermometer Temperature Humidity Meter Gauge Hygrometer

Digital Humidity Temperature Gauge, Thermometer Hygrometer Meter. Indoor with Alarm Clock

Characteristic:

1.Large LCD display.Show the indoor temperature/humidity and time at the same time.

2. Alarm function.

3.12/24 hour display switching function

4."℃ / ℉" display switching function.

5. Highest / lowest indoor temperature and humidity memory function.

6.Products with Supporting plate and hanging hole ,can be placed in vertical or hanging

Product parameters:

Temperature survey range:: 0℃-50℃(32℉-122℉)

Humidity survey range : 10%- 98%

Analyze degree: 0.1℃, 1%RH

Accurate precision: ±1℃, ±5%RH

Power Supply: one AAA battery

The button usage:

* "MODE"

1 , press once to switch the display time and the alarm time ( two dots without flashing ) .

2 ,Time and Date setting

When displaying the time mode, press and hold 2 seconds to enter time setting , set the minute, hour, 12/24 hour mode , month, day . During the time digits flash , press "ADJ" to adjust. When completed a set , and then press the "MODE" key once , the next one will be automatically set . If one minute without any key operation , it will automatically exit setup,and finish setting.

3 ,Alarm setting

When displaying the alarm time (AL) mode , press and hold 2 seconds to enter the alarm time setting , the same operation mode and time settings .

* "ADJ"

1,When setting time , date, alarm, you can make the data increases, Press and hold the button to increase rapidly.

2 , When displaying the alarm time (AL) mode , press the ADJ adjustable alarm off. ( When Alarm function is turned on, the screen has a bell icon ) .

* "MAX / MIN"

1 , Press "MAX / MIN" key once to display the maximum period of MAX- measuring indoor temperature and humidity ; then press the "MAX / MIN" key once to display the minimum measurement period MIN- indoor temperature and humidity .

* "℃ / ℉"

1 , the black key is located on the back of the meter. press "℃ / ℉" key, you can choose to display temperature in Celsius or Fahrenheit .

Package Include:

1 x Indoor Outdoor Digital Thermometer Hygrometer